Three Rivers Gallery & Gifts Exhibit Regulations

2D ARTWORK FRAMING REQUIREMENTS

1. Select a Frame

Consider creating work that will fit in standard-sized mats and frames.

* Showcase your artwork and not the frame! Simple mats and frames are just fine!
* Canvases must be framed or gallery wrapped.

2. Choose correct hardware for the back of your work

* Please use good D-rings, larger screw eyes, metal-frame D-rings, all securely installed.
Examples of *Acceptable Hooks*:

|  |  |  |  |
| --- | --- | --- | --- |
| Hook1 | Hook 2 |  | Hook 4 |

* Please, no clip-frames, saw-tooth hangers, a single triangle hanger at the center, back of frame, triangle hangers/wires that are not attached to the sides of frames, very small screw eyes or corded backs Examples of *Unacceptable Hooks*:

|  |  |  |  |
| --- | --- | --- | --- |
| Bad Hook 1Clip Frame | Bad Hook 2Saw-Tooth Hangers | Bad Hook 3Wire Not Attached to Frame | Bad Hook 4Hanger Not Attached to Frame |

3. Hanging wire

* For the safety of your artwork, please use quality picture hanging wire.
* Please refrain from using fishing line, electric wire and mesh cord.

|  |  |  |  |
| --- | --- | --- | --- |
| Quality WireQuality Picture Hanging Wire | Fishing WireNo Fishing Line | Electical WireNo Electrical Wire | Corded WireNo Corded Wire |

4. Attaching hardware and hanging wire to the backs of frames:

* When adjusting your hanging wire, make sure to leave plenty of lead to wrap around the wire after looping your D-Ring or screw eye—it is more secure that way.
* We recommend looping your D-Ring hardware twice for increased safety of your artwork.
* Tape all ends of wires so it does not cut the 2D displayer.

|  |  |  |
| --- | --- | --- |
| Good Attachment 1Lead wire securely wound around D-Ring | Good Attachment 2Double Loop through D=Ring | Good Attachment 3Secure lead through ring tightly wound |
| Bad Attachment 1Short lead wire can come apart | Bad Attachment 2Loose wrap can unravel | Bad Attachment 3Short wire not cleanly wound and fraying |

* **Please make sure that your D-rings are attached correctly on your frame. Best practice is to have the D-rings attached 1/3 of the way down your frame.**
* **Your hanging wire should be long enough so that, when pulled up tight, the top of the wire is about 2” from the top of the frame.**

|  |
| --- |
| Correct Picture Back |

5. Labeling your work…even if you sign the front!

* Please attach a small card that displays your full contact information and the title of each work securely to the back of your artwork. You will also display the TRAG inventory tag with price.

6. Clean your artwork before your exhibit—this will be the first time that many viewers are introduced to your work and to you as the artist. Make a good first impression!

* Dust off your work, remove fingerprints from the glass, clean out any dirt and repair any damage on the outside AND inside of your work.
* Make sure any mats are pressed snugly to the glass or Plexiglas and are not crooked in the frame, “bubbling” out or loose in the frame.